# How to Read a Mold Inspection Report (2026 Guide)

**Slug:** `how-to-read-a-mold-inspection-report`
**Read time:** 12 min read
**Author:** Mike Nguyen

_Learn how to read a mold inspection report. Understand air sample results, spore counts, species identification, and what the numbers actually mean for your nex_

---

<h1>How to Read a Mold Inspection Report</h1>

  <p>A mold inspection report shows three things: species identified, sample locations, and concentration levels. Start with the species identification section. Then compare indoor spore counts to the outdoor baseline sample. The species matter more than the numbers alone — a small amount of Stachybotrys chartarum is a different problem than a large amount of Cladosporium.</p>

  <p>Most reports arrive as a 10-30 page PDF with lab data, inspector notes, and recommendations. The format varies by lab, but the core sections are consistent. You want to understand what was found, where it was found, and what it means for your property.</p>

  <h2>What's Included in a Mold Inspection Report</h2>

  <p>A standard mold inspection report contains five sections: inspector credentials and visit details, sample location descriptions, laboratory analysis results, species identification, and recommended next steps. Some labs include photos of sampling locations. Most AIHA-EMPAT certified labs organize the data the same way.</p>
  <aside class="callout-info" data-fmt-injected="lm-v1" data-cta-id="lm-lm-inspection-guide-post-intro" data-position="post-intro">
    <p><strong>Need to go deeper?</strong> Detailed walkthrough of FMT's inspection process. Lead magnet for inspection-process and mold-types-detection clusters.</p>
    <p><a href="https://fastmoldtesting.com/inspection-guide?utm_source=seo&amp;utm_medium=article&amp;utm_campaign=lead-magnet&amp;utm_content=lm-lm-inspection-guide-post-intro">Read: Mold Inspection Guide</a></p>
  </aside>


  <p>Here's what each section covers:</p>

  <ul>
    <li><strong>Inspector information</strong> — IICRC or NORMI certification, company name, inspection date, property address</li>
    <li><strong>Sample locations</strong> — where each air or surface sample was taken (master bedroom, attic, HVAC return, exterior control)</li>
    <li><strong>Lab results</strong> — spore counts in spores per cubic meter (spores/m³) for air samples, or colony forming units (CFU) for surface samples</li>
    <li><strong>Species identification</strong> — which mold types were found in each sample, identified by genus or species name</li>
    <li><strong>Recommendations</strong> — what to do based on findings, from "no action needed" to "remediation recommended"</li>
  </ul>

  <p>Reports from <a href="https://fastmoldtesting.com/services/mold-inspection">certified mold inspectors</a> also include an outdoor control sample. That baseline is how you judge whether indoor levels are elevated.</p>

  <h2>Understanding Air Sample Results</h2>

  <p>Air samples measure mold spore concentration in the air you breathe. Results are reported in spores per cubic meter (spores/m³) — a count of how many mold spores were captured in the lab analysis of the air sample.</p>

  <p>The outdoor control sample is the reference point. If your outdoor sample shows 500 spores/m³ and your living room shows 450 spores/m³, that's normal. If your living room shows 2,000 spores/m³, that's elevated.</p>

  <p>Here's a sample comparison:</p>

  <div style="overflow-x:auto">
    <table>
      <thead>
        <tr>
          <th>Sample Location</th>
          <th>Total Spores/m³</th>
          <th>Dominant Species</th>
        </tr>
      </thead>
      <tbody>
        <tr>
          <td>Outdoor (control)</td>
          <td>650</td>
          <td>Cladosporium, Ascospores</td>
        </tr>
        <tr>
          <td>Living room</td>
          <td>580</td>
          <td>Cladosporium, Penicillium</td>
        </tr>
        <tr>
          <td>Master bedroom</td>
          <td>1,850</td>
          <td>Aspergillus, Penicillium</td>
        </tr>
        <tr>
          <td>Basement</td>
          <td>3,200</td>
          <td>Stachybotrys, Chaetomium</td>
        </tr>
      </tbody>
    </table>
  </div>

  <p>In this example, the living room is fine. The master bedroom is elevated. The basement is a problem — both the count and the species (Stachybotrys + Chaetomium are water-damage indicators).</p>

  <p>Labs report spore counts by genus or species. The total count tells you concentration. The species breakdown tells you what's growing and why.</p>

  <p>Most air samples capture between 200 and 2,000 spores/m³ indoors. Outdoor samples in summer can run 2,000-10,000 spores/m³ depending on region and season. Context matters more than any single number.</p>

  <h2>Decoding Surface Sample Results</h2>

  <p>Surface samples test what's growing on walls, HVAC vents, or other materials. Results are reported in colony forming units (CFU) instead of spores/m³. A CFU is a viable mold colony that grew on the lab's culture plate after they incubated your sample.</p>

  <p>Surface sample methods include:</p>

  <ul>
    <li><strong>Tape lift</strong> — clear tape pressed against a surface to capture spores and fragments</li>
    <li><strong>Swab sample</strong> — sterile swab rubbed across a defined area</li>
    <li><strong>Bulk sample</strong> — piece of material (drywall, insulation, carpet) sent to the lab</li>
  </ul>

  <p>Surface samples tell you what's on a specific spot. They don't tell you air quality. A surface can test positive for mold without affecting the air — or the air can be contaminated even when visible surfaces look clean.</p>

  <p>Use surface samples to confirm visible mold, identify hidden growth behind walls, or verify cleanup after remediation. Air samples measure the bigger picture — what you're breathing.</p>

  <h2>Species Identification — What Each Type Means</h2>

  <p>The species list matters more than the spore count. Some species indicate water damage. Some are common outdoor mold that blew in through open windows. Some produce mycotoxins under certain conditions.</p>

  <p>Here's what the most common species mean:</p>

  <div style="overflow-x:auto">
    <table>
      <thead>
        <tr>
          <th>Species</th>
          <th>Where It Grows</th>
          <th>What It Indicates</th>
        </tr>
      </thead>
      <tbody>
        <tr>
          <td><strong>Aspergillus</strong></td>
          <td>Damp materials, HVAC systems, walls with moisture intrusion</td>
          <td>Water damage or high humidity. Some species produce mycotoxins. Common indoors.</td>
        </tr>
        <tr>
          <td><strong>Penicillium</strong></td>
          <td>Water-damaged drywall, carpet, wallpaper, insulation</td>
          <td>Active or recent water damage. Grows fast on wet cellulose materials.</td>
        </tr>
        <tr>
          <td><strong>Stachybotrys chartarum</strong></td>
          <td>Chronically wet cellulose (drywall, wood, paper)</td>
          <td>Chronic water intrusion. This is "black mold." Produces mycotoxins. Needs remediation.</td>
        </tr>
        <tr>
          <td><strong>Cladosporium</strong></td>
          <td>Outdoor air, HVAC filters, window frames</td>
          <td>Usually outdoor mold. High indoor counts suggest poor ventilation or open windows during sampling.</td>
        </tr>
        <tr>
          <td><strong>Chaetomium</strong></td>
          <td>Very wet drywall, wood, ceiling tiles after long-term leaks</td>
          <td>Severe water damage, often structural. Needs immediate remediation.</td>
        </tr>
        <tr>
          <td><strong>Alternaria</strong></td>
          <td>Outdoor air, damp bathrooms, window sills</td>
          <td>Common outdoor allergen. High indoor levels suggest ventilation problems.</td>
        </tr>
      </tbody>
    </table>
  </div>

  <p>If your report shows Stachybotrys or Chaetomium, you have a water problem that needs fixing. If it shows mostly Cladosporium and Alternaria matching outdoor levels, you're fine.</p>

  <p>The AIHA-EMPAT certified lab that analyzed your sample identified species using microscopy or DNA sequencing. <a href="https://www.aiha.org/">AIHA</a> (American Industrial Hygiene Association) sets the EMPAT certification standard for mold analysis labs. Some species look identical under a microscope — DNA sequencing (used by AI-assisted lab analysis at <a href="https://fastmoldtesting.com/services/mold-testing">Fast Mold Testing</a>) is more accurate.</p>

  <h2>What the Numbers Actually Mean</h2>

  <p>There's no universal threshold for "safe" vs "dangerous" mold levels. The <a href="https://www.cdc.gov/">CDC</a> and <a href="https://www.epa.gov/">EPA</a> don't publish cutoffs because safe levels vary by species, exposure duration, and individual sensitivity.</p>

  <p>Instead, compare indoor levels to your outdoor baseline. Three patterns matter:</p>

  <ol>
    <li><strong>Indoor lower than or equal to outdoor</strong> — normal. Mold spores blow in from outside. If your indoor count matches outdoor, you don't have an indoor source.</li>
    <li><strong>Indoor 2-3x outdoor</strong> — minor elevation. Check for humidity problems, improve ventilation, monitor. Not usually remediation-level.</li>
    <li><strong>Indoor 5x+ outdoor, or presence of water-indicator species</strong> — significant finding. Remediation recommended.</li>
  </ol>

  <p>Example: outdoor shows 800 spores/m³ of mixed species. Your bedroom shows 850 spores/m³ of the same species. That's fine. Your basement shows 4,500 spores/m³ with Stachybotrys and Penicillium. That's a problem.</p>

  <p>Some labs add "risk" categories (low, moderate, elevated, high) to their reports. Those categories are lab-specific — not standardized. Read the species and the indoor/outdoor ratio yourself.</p>

  <p>Also check for diversity. Finding 6+ species in one sample location often means multiple moisture sources or long-term water damage.</p>

  <h2>Red Flags to Look For</h2>

  <p>These patterns in a mold report mean you need action:</p>

  <ul>
    <li><strong>Stachybotrys chartarum at any level</strong> — indicates chronic water damage, produces mycotoxins, needs remediation</li>
    <li><strong>Indoor count 5x or higher than outdoor</strong> — you have an active indoor mold source</li>
    <li><strong>Water-indicator species</strong> (Stachybotrys, Chaetomium, Fusarium, Ulocladium) — these only grow on very wet materials</li>
    <li><strong>Multiple species in one location</strong> — suggests long-term moisture or multiple moisture events</li>
    <li><strong>Elevated levels in HVAC samples</strong> — mold in your air handler spreads spores throughout the house</li>
  </ul>

  <p>If your outdoor sample shows 200 spores/m³ and your attic shows 15,000 spores/m³, don't wait for a second opinion. You have an attic problem.</p>

  <p>Also watch for species that don't match outdoor. If outdoor shows mostly Cladosporium and Alternaria, but indoor shows Aspergillus and Penicillium, those are growing indoors.</p>

  <h2>What to Do After You Read Your Report</h2>

  <p>Your next steps depend on what the report found.</p>

  <p><strong>Clean report (indoor ≤ outdoor, common species only):</strong><br>
  No remediation needed. Keep humidity below 50%, fix any leaks promptly, change HVAC filters regularly.</p>

  <p><strong>Minor elevation (indoor 2-3x outdoor, no water-indicator species):</strong><br>
  Improve ventilation, run dehumidifiers, identify and fix minor moisture sources (leaky faucet, bathroom exhaust). Retest in 30-60 days to confirm levels drop.</p>

  <p><strong>Significant finding (indoor 5x+ outdoor, or Stachybotrys/Chaetomium present):</strong><br>
  Remediation needed. Hire a licensed mold remediation company. Do NOT hire the same company that did your testing — that's a conflict of interest. Fix the water source first (roof leak, plumbing, foundation drainage) or the mold will return.</p>

  <p><strong>Unclear or borderline results:</strong><br>
  Get a second opinion from an independent inspector. At <a href="https://fastmoldtesting.com/about">Fast Mold Testing</a>, we don't remediate — so the report is straight. If your first inspector also sells remediation, the second opinion matters.</p>

  <p>Post-remediation, retest before closing up walls. Confirm spore counts dropped to normal and water-indicator species are gone.</p>

  

  <h2>Conclusion</h2>

  <p>Focus on three things when you read a mold report: species identified, indoor vs outdoor comparison, and whether water-indicator species are present. The numbers matter, but context matters more. A report showing Cladosporium at 1,800 spores/m³ matching outdoor is fine. A report showing Stachybotrys at 200 spores/m³ is not.</p>

  <p>If your report shows elevated levels or water-damage species, fix the moisture source and hire a remediator. If it's borderline, improve ventilation and retest in 60 days.</p>

  <p>Need an inspection with <a href="https://fastmoldtesting.com/pricing">1–2 business days lab results</a> and a report you can actually understand? Fast Mold Testing uses AI-assisted lab analysis for species ID and delivers interactive web reports — not 30-page PDFs. Book online in under two minutes.</p>

## FAQ

**Q: What is a normal mold spore count indoors?**
A: Normal indoor spore counts range from 200 to 2,000 spores/m³, depending on outdoor levels and season. The key is whether indoor matches outdoor. If outdoor is 1,500 spores/m³ and indoor is 1,400 spores/m³, that's normal. If outdoor is 400 and indoor is 2,500, that's elevated.

**Q: How do I know if my mold levels are dangerous?**
A: Compare indoor spore counts to outdoor baseline. If indoor is 5x outdoor or higher, or if your report shows Stachybotrys chartarum, remediation is recommended. Also check for symptoms — persistent cough, headaches, or respiratory issues that improve when you leave the property.

**Q: What does Stachybotrys on my report mean?**
A: Stachybotrys chartarum (black mold) grows on chronically wet cellulose materials like drywall and wood. It produces mycotoxins. Finding it means you have a long-term water problem that needs remediation. Fix the water source, remove contaminated materials, retest to confirm clearance.

**Q: Why does the report compare indoor to outdoor samples?**
A: Mold spores are always in outdoor air. They blow indoors through windows, doors, and HVAC systems. Comparing indoor to outdoor tells you whether you have an indoor mold source or just normal outdoor spores. If indoor is lower than outdoor, you don't have a problem.

**Q: How long is a mold inspection report valid?**
A: Most reports are valid for 30-90 days. Mold grows fast when moisture is present — a clean report today doesn't guarantee clean conditions in six months. If you had a new leak, flood, or humidity problem since the inspection, retest. Use the report for immediate decisions, not long-term assurance.
